* J1. PJ-059AH
  + <https://www.cuidevices.com/product/resource/pj-059ah.pdf>
* LM317\_TO-220
  + Package\_TO\_SOT\_THT:TO-220-3\_Vertical
  + http://www.ti.com/lit/ds/symlink/lm317.pdf
* U1 : LM7805\_TO220
  + Package\_TO\_SOT\_THT:TO-220-3\_Vertical
  + <https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF>
* C1 : 10μF :
  + Capacitor\_SMD: C\_0805\_2012Metric
  + πάνω από 12V
* C2 : 0,1 μF :
  + Capacitor\_SMD: C\_0805\_2012Metric
  + πάνω από 5V
* C3 : 1 μF :
  + Capacitor\_SMD: C\_0805\_2012Metric
  + πάνω από 5V
* R1 : 180Ω
  + Resistor\_SMD:R\_0805\_2012Metric
* R2 : 330Ω
  + Resistor\_SMD:R\_0805\_2012Metric
* R3 : 560Ω
  + Resistor\_SMD:R\_0805\_2012Metric
* D1 : LED
  + LED\_SMD:LED\_0805\_2012Metric
* J4 : Screw\_Terminal\_01x06
  + TerminalBlock:TerminalBlock\_bornier-6\_P5.08mm
  + <https://www.snapeda.com/parts/CTB0700/3/Camden%20Boss/datasheet/>
* J6 : Conn\_01x03\_Male
  + Connector\_PinHeader\_2.54mm:PinHeader\_1x03\_P2.54mm\_Vertical
* J7 : Screw\_Terminal\_01x02
  + TerminalBlock:TerminalBlock\_bornier-2\_P5.08mm
  + <https://www.snapeda.com/parts/CTB0700/3/Camden%20Boss/datasheet/>
* J13 : Conn\_01x04
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x04\_P2.54mm\_Vertical
* J11 : Conn\_01x12
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x12\_P2.54mm\_Vertical
* J2 : Conn\_01x7
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x7\_P2.54mm\_Vertical
* J8 : Conn\_01x5
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x5\_P2.54mm\_Vertical
* J12 : Conn\_01x4
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x4\_P2.54mm\_Vertical
* J14 : Conn\_01x4
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x4\_P2.54mm\_Vertical
* J5 : Conn\_01x4
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x4\_P2.54mm\_Vertical
* J10 : Conn\_01x4
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x4\_P2.54mm\_Vertical
* J9 : Conn\_01x7
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x7\_P2.54mm\_Vertical
* J3 : Conn\_01x8
  + Pinsockets – female
  + Connector\_PinSocket\_2.54mm:PinSocket\_1x8\_P2.54mm\_Vertical

